Lab Exercise 3: Wireshark Installation and Introduction

1. 74 bytes
2. Destination: 1a:e8:29:53:a6:a0, Source: dc:1b:a1:45:2c:ca
3. IntelCor
4. Type: IPv4 (0x0800)
5. 0100 .... = Version: 4, Header Length: 20 bytes (5)
6. Source Address: 192.168.157.121, Destination Address: 23.93.76.124
7. Type: 8 (Echo (ping) request), Type: 0 (Echo (ping) reply)
8. 