A screenshot of a computer

Description automatically generated

1. IPv4 address: 172.16.10.111.

Class: B

1. Subnet Mask: 255.255.255.0/24

Default Mask: No, 8

Subnet Number: 172.16.10.0

1. Default Gateway: Yes, 172.16.10.1
2. DHCP: Yes, 172.16.10.1

Lease Length: Wednesday, September 13, 2023 - Friday, September 15, 2023

1. 4f:64:f6
2. 0x0806
3. Broadcast, it says so in the destination
4. No, no
5. Request(1)
6. To get the mac address of the device at the IP address 172.16.10.111
7. Reply
8. Unicast
9. DC-1B-A1-45-2C-CA
10. UDP
11. Broadcast, says so in the destination
12. Boot Request (1)
13. DHCP Discover (1)

A screenshot of a computer

Description automatically generated

A screenshot of a computer

Description automatically generated